ANNOUNCING:  NEW version 2.53

DEMO version for Series 3/3a/Workabout now available to try before you buy! 
Just copy PCOMDEMO.app onto your Psion computer and install it as an APP on your ICON screen, and then run it.  The demo only runs at 300 baud, and does not allow any file/config saves, but everything else will function to allow you to test drive it.  
(Real version installs under Windows 3.x with Psion serial cable).

NEW FEATURES in 2.53 version:

 	Workabout version added 
 	3270 emulation (like IBM's FTTERM) to connect to IBM hosts
 	Supports barcode scanning on the HC in VT100 mode
 	Diagnostic support for RS232 technical troubleshooting
 	Screen capture and Logging to save your E‑Mail, etc.
 	Reverse Screen Image
	Plus, all of the features already in 2.4x versions
	
©1993,5 Advanced Systems Consultants, Inc. (ASC)
	
Running on the PSION SIBO family of products, this software product provides "easy‑to‑use" PC‑like communications software for the HC, Series 3/3A, and the new Workabout.  Using the terminal emulation, you can connect to the outside world of PC host systems, Unix systems, BBS networks, Compuserve, or any RS‑232 asynchronous host.  Using the file transfers, you can upload or download files using full error‑checking protocols such as XMODEM or YMODEM to insure 100% data integrity.  You can create "Scripts" for logging into host systems automatically.  Further, these same scripts can be used directly with ProComm+ 2.0 for testing and debugging! 

A dialing directory is included so that you can easily have a database of names on file with telephone numbers and parameters for each dialing entry. The whole package is written in 'C' for extremely fast operation, total low‑level hardware control, and designed to use as little memory as possible to allow for programmer calls.  It supports all standard Psion serial interfaces including EXTECH, Dynasys, and Psion 3FAX modem.  All functions use a simple PC‑like hot‑key approach such as  the Psion key (lock) plus "H" key for "Help"; the dialing directory is "Psion + D", etc.

APPLICATIONS:
PCOMM(tm) can be used for remote dial‑in‑access to update databases, get messages or files, download or upload a current price list or inventory file, control RS‑232 devices, emulate a host  terminal, call BBS systems, and many more.  If you are writing code for a Psion terminal, you can call PCOMM(tm) with a script file from OPL/G or 'C' for total communications control.  Write your applications in OPL/G or 'C', collect the data, and then pass control to PCOMM(tm) to dial host systems to upload all collected data.  

FEATURES:

TERMINAL EMULATION:  PC‑ANSI, VT100, or  IBM 3270.  VT100 emulation can be used with many host mainframes.  ANSI would be used for PC mode emulations, and 3270 supports IBM mainframe: CICS, VTAM, and PROFS!, etc.  PCOMM(tm) supports screen control characters as well as function keys such as PF1, F1, etc.  Series 3A features a 25x80 screen, or, you can use our scrolling virtual window.  PCOMM(tm) was designed especially for small screen terminals.

FILE TRANSFERS:  Supports XMODEM, YMODEM (and YMODEM batch), and ASCII protocols.

DIALING DIRECTORY:  A database of names (limited only by disk space) includes telephone numbers, dialing parameters with port setups for each entry which also allows for multiple serial ports on your Psion HC terminal. Supports international dialing and most PBX systems.

HAYES MODEM COMPATIBLE:  Uses standard Hayes Modem commands, but you can choose your own modem initialization string.  Configuration file allows you to select 300‑19200 baud rates, 7 or 8 data bits, l or 2 stop bits, ODD, EVEN, or NO parity, and Port A, B, Cradle, D, or E, etc.

HOT KEYS:  like the PC ALT  key, use the PSION(LOCK) key for fast execution on commands as well as ease of use.  Some more examples of Psion hot keys:
(Utilizes least keystrokes possible.)
	(diamond) + 1 = F1/PF1 for IBM Hosts			(diamond) + 2 = F2/PF2
	PSION + S = Setup Configuration				PSION + P = Port setup
	PSION + U = upload file					PSION + W = download file
	CTRL + (UP ARROW) = scroll up virtual window	
	CTRL + (DN ARROW) = scroll down virtual window

SCRIPTING MODE:  We consider this our most powerful feature as you can fully automate all of your communications with this.  You can execute the script by typing "PCOMM scriptname.ASP" where scriptname is a standard ASCII text file, or execute the script file from within PCOMM(tm) with one hot‑key.  The script file also works directly with ProComm+ 2.0 (when compiled with ProComm+) which is great when used as a development tool.  Scripting can be used to automatically log into BBS systems using passwords, log into your own host systems for file transfers, check EMAIL, etc.  It's only limited by your creative imagination.

MACRO KEYS:  allow custom key mapping, special codes, even execute script files with this feature.

3270 EMULATION:  allows remote connection to an IBM mainframe such as a 3090 or ES9000 and you can run PROFS, CICS, VTAM, etc.

DIAGNOSTICS MODE:  allows visual verification of the line status for RTS, CTS, DSR, DTR, DCD as well as modification of DTR.

SCREEN CAPTURE:  allows screens to be captured to a file on your Psion computer.

To order PCOMM(tm), contact the distributor nearest you or contact us for your nearest distributor.  
Ask your local dealer/distributor about our many other fine software products:
 	RF Library Communications (Radio Frequency)
 	RF Communications, Custom, Narrow and Spread Spectrum.
 	PC Gateway 16‑port Host to Psion communications server (DOS version)
 	Psion System Customization and Integration, especially Inventory 	Control, Warehouses, mainframe connectivity.  (AS/400, 3090, HP,  DEC, etc.)

PCOMM(tm) PRICE: £75.00 + £6.00 shipping and handling (U.K. Pounds excluding VAT, price subject to change without notice). Supplied on 3.5" diskettes with documentation, unique serial number for technical support, registration certificate, and 90 days of free inbound telephone support and upgrades.  You must specify HC, or Workabout / Series 3A.  Group discounts, special configurations, SSD media, or customization may be requested.  (PCOMM(tm) is protected under USA and International copyright laws and is licensed per single Psion computer unless a site license is obtained.) 

MERCURY CONTROL LIMITED accepts Personal Checks, Company Checks, Purchase Orders with approved credit, Money Orders, etc.  Approved Credit orders will be shipped the same day order is received, others on the day payment is received.

	©1993,5 Advanced Systems Consultants, Inc. (ASC)
	Distributed in the UK by :-	MERCURY CONTROL LIMITED
43 Clarendon Road
Leeds  LS2 9NZ
					T. 0113 244 3301
					F. 0113 244 3302
					M. 0973 639 688

Installation requires a serial port on the Psion computer, and Windows 3.1x running on a PC.  Pre‑installation on an SSD is an additional £30.00  (U.K. Pounds excluding VAT, price subject to change without notice).

Upgrades after 90 days are £25.00 plus £6.00 shipping and handling  (U.K. Pounds excluding VAT, price subject to change without notice).  Any version update prior to version 2.50 requires a diskette upgrade.  If you have version 2.50 or greater, upgrades can be provided via Compuserve.  Our Compuserve address is 100142,1665.

Requested emergency orders incurr the carrier's overnight shipping fees. 

(This software and all documentation is copyrighted by ASC.  PSION, HAYES, IBM, DEC, ProComm+, & EXTECH are trademarks of their respective companies)

<<-------------------- End of Document -------------------->>